**Q1)** In this question discrete time step calculations in the simulation of a single-phase uncontrolled rectifier that is feeding a resistive load (R=100Ω) is performed. Simulation results with step size 1.5 msec, 10 µsec and 1 µsec can be observed in Figure 1, 2, and 3, respectively.





